Automotive Qualification Results Summary for Die Revision of ADSP-BF70x Blackfin Processors

|  |
| --- |
| **Qualification Result** |
| Test | Conditions | Sample Size | Results |
|

|  |
| --- |
| Electrostatic Discharge*Field Induced Charge Device Model* |

 | **JESD22**-C101 | **3/voltage** | **Pass** ±500V all pin, pass ±750V corner pin |
| Electrostatic Discharge*Human Body Model* | **ESDA/JEDEC** JS-001-2011 | **3/voltage** | **Pass** ±2000V |
| Latch-Up  | **JEDEC**-JESD78 | **1x12** | **Pass** ±200mA  |