|  |
| --- |
| ADSP-BF504 Die Revision 0.1 QUALIFICATION RESULTS |
| Test | Conditions | Sample Size | Results |
| Latch-Up | JEDEC *JESD78**Class II, Level A* | **6** | **Pass** |
| Electrostatic Discharge*Human Body Model* | ESDA/JEDEC*JS-001-2011* | **3/voltage** | **Pass ±4000V** |
| Electrostatic Discharge*Field-Induced Charged Device Model* | JEDEC*JESD22-C101* | **3/voltage** | **Pass ±1250V** |

|  |
| --- |
| ADSP-BF504F Product Revision 0.1 QUALIFICATION RESULTS |
| Test | Conditions | Sample Size | Results |
| Latch-Up | JEDEC *JESD78**Class I, Level A* | **6** | **Pass** |
| Electrostatic Discharge*Human Body Model* | ESDA/JEDEC*JS-001-2011* | **3/voltage** | **Pass ±4000V** |
| Electrostatic Discharge*Field-Induced Charged Device Model* | JEDEC*JESD22-C101* | **3/voltage** | **Pass ±1250V** |