|  |
| --- |
|  |

**Qualification Results Summary of**

**ADP2119/20 Die Revision B Qualification**

|  |  |  |  |
| --- | --- | --- | --- |
| **QUALIFICATION RESULT** | | | |
| **Test** | **Specification** | **Sample Size** | **Result** |
| Electrostatic Discharge  *Field-Induced Charged*  *Device Model* | JEDEC*JS-002* | 3/voltage | PASS ±TC1250 |
| Electrostatic Discharge  *Human Body Model* | JEDEC *JESD22-A114* | 3/voltage | PASS ±4000V |
| Latch-Up | JEDEC *JESD78* | 15 | PASS |
| Solder Heat Resistance (SHR)1 | JEDEC *J-STD-020* | 30 | PASS |

1Preconditioned per JEDEC J-STD-020 Level 3